Summary Drawing Report
T:/Piotr_Przystup/TEXAS_INSTRUMENTS/ZLL_REMOTR/PCB/ZLL_RC.brd
Tue Apr 02 13:36:04 2013
Drawing Statistics:
    Drawing Extents  XL(-200.0000)  YL(-200.0000)  XU(800.0000)  YU(800.0000)
    Dimensions in millimeters with 4 decimal places
    Package Symbols:  Total(72)  Mirrored(52)  Embedded(0)  Pins(205)
    Mechanical Symbols:  Total(0)  Mirrored(0)  Pins(0)
    Format Symbols:  Total(1)
    DRC State: UP TO DATE
    DRC Errors: 0
    Short DRC: 0
    Waived DRC: 60
    Padstack Definitions: 115
    Functions:   Assigned(73)  Unassigned(0)  Total(73)

Connection Statistics:
    Connections:  W/Rats(140)  No/Rats(0)  Total(140)
    Already Connected:  W/Rats(140)  No/Rats(0)  Total(140)
    Missing Connections: W/Rats(0)  No/Rats(0)  Total(0)
    Dangling Connections (See logfile):  0
    Connection Completion:  W/Rats(100.00%)  No/Rats(0.00%)  Total(100.00%)  
    Manh Distance (cm):  100.8509
    Etch Length (cm):  W/Rats(129.13)  No/Rats(0.00)  Total(129.13)
    Number of Vias:  W/Rats(776)  No/Rats(0)  Total(776)
    Vias per Connection:  W/Rats(5.54)  No/Rats(0.00)Total(5.54)
    SMD pins with attached clines:  175

Layout Statistics:
    Components:  Placed(70)  Unplaced(0)  Total(70)
    Nets: W/Rats(40)  No/Rats(0)  Total(40)
    Pins: W/Rats(180)  No/Rats(0)  Unused(19)  Unplaced(0)  Total(199)
    Equivalent ICs (1 pin = 1/14 EIC):  14
    RatTs:  0
    Router Keepin (cm):   (0.0500,0.0500) by (3.5079,7.9801)
    Layout area (sq cm):  26.95
    Average ratlength (cm):   0.7
    Rat density (cm/sq cm):  3.742
    Double-sided rat density (cm/sq cm):  1.871

Layout/Pin Density Statistics
Layer,Layout Area<BR>(sq cm),Components,Pins,Layout Density<BR>(sq cm/EIC),Pin Density<BR>(pins/sq cm)
External(Double-Sided),53.90,72,205,3.681,3.803
Embedded(0),0.00,0,0,0.000,0.000
Design,26.95,72,205,1.841,7.607

Etch Layer Statistics:
Layer,Clines/Carcs,Shapes(voids),Rectangles,Lines/Arcs,Text,Components(Pins)
TOP,67,4(16),0,0,0,20(34)
BOTTOM,212,15(17),0,0,0,52(171)

