
Company Name:		TEXAS INSTRUMENTS
PC Board Name:		F28PLC90PZT_AFE032      
PC Board Number:		F28PLC90PZT_AFE032 
Revision:			1
Design House:		Willow Spring Technical Services, Corp.
Job Number: 		TEX132

Designed by:          		Carl Sangiolo
Contact Number:       	(508) 947 - 2709
e-mail:              		carl@wstscorp.com
Files Included:
	
Filename			Description					Format
--------			-----------						------
L1.PHO			Primary Side Cu					Gerber 8.5
L2.PHO			Internal Plane 1 (NEG)		          		Gerber 8.5
L3.PHO			Internal Plane 2 (NEG)				Gerber 8.5
L4.PHO			Secondary Side Cu					Gerber 8.5
PSS.PHO			Primary Silkscreen A/W				Gerber 8.5
SSS.PHO			Secondary Silkscreen A/W       			Gerber 8.5
PSM.PHO			Primary Soldermask A/W				Gerber 8.5
SSM.PHO			Secondary Soldermask A/W 				Gerber 8.5
PST.PHO			Primary Solder Stencil A/W 				Gerber 8.5
SST.PHO                 		Secondary Solder Stencil A/W    	       		Gerber 8.5
DD.PHO			Drill Drawing  					Gerber 8.5
NC_DRILL.DRL		NC Drill Data					NC DRILL ASCII																
NC_DRILL.REP		Drill Tool Listing					ASCII
NC_DRILL.LST		Drill X-Y Listing					ASCII
IPCD356.NET		IPC-D-356 Netlist					IPC-D-356 ASCII
README.TXT   		This File						ASCII





NOTES: 

1) USE FILM OUTLINE CORNERS TO ALIGN ARTWORKS

2) ALL THERMALS ARE O.D.  I.D.= O.D. - .020
   WITH A .015 OPEN AT 45 DEGREES.

3) ALL VIAS SHALL HAVE A DIRECT CONNECTION
   TO THE PLANE. NO THERMALS ON VIAS.
